communication - SendToEnv

Page / - last modified by Outhman Moustaghfir on 2024/01/22 16:19

SendToEnv

last modified by Outhman Moustaghfir

on 2024/01/22 16:19

Table of Contents

Definition

Icon

Configuration

1- Configuration of SendToEnv

Definition

The SendToEnv Connector streamlines the transfer and management of files across multiple environments in a network. It ensures efficient, automated file movement, integral to workflow optimization.

Icon

Configuration

1- Configuration of SendToEnv

you can configure SendToEnv and put the correct data:

For Example:

File(s): Specifies the file or files to monitor for transfer.

Environments: Lists the target environments where the files will be sent. Multiple environments can be separated by ";".

Example: iXPath;Centrale_Danone.

Mask: Defines the pattern to filter the files that this connector should handle. The .* mask indicates that all files are included.

Log Level: Determines the verbosity of the logs for this connector. The level DEBUG implies detailed logging which is useful for troubleshooting.

Condition: Allows specifying a condition that must be met for the connector to process the files.

Add boundary OnError: When checked, this option may add additional error handling, such as transaction boundaries, to manage failures gracefully.