communication - SendToEnv 

Page / - last modified by Outhman Moustaghfir on 2024/01/22 16:54 

SendToEnv 
last modified by Outhman Moustaghfir
on 2024/01/22 16:54

Table of Contents
Definition
Icon
Configuration
1-  Configuration of SendToEnv

Definition
The SendToEnv Connector streamlines the transfer and management of files across multiple environments in a network. It ensures efficient, automated file movement, integral to workflow optimization.
Icon
 
Configuration
1-  Configuration of SendToEnv
you can configure SendToEnv and put the correct data:
For Example:

File(s):  Specifies the file or files to monitor for transfer.
Environments:  Lists the target environments where the files will be sent. Multiple environments can be separated by ";". 
                                             Example:   iXPath;Centrale_Danone.
Mask:  Defines the pattern to filter the files that this connector should handle. The .* mask indicates that all files are included.
Log Level:  Determines the verbosity of the logs for this connector. The level DEBUG implies detailed logging which is useful for troubleshooting.
Condition:  Allows specifying a condition that must be met for the connector to process the files. 
Add boundary OnError:  When checked, this option may add additional error handling, such as transaction boundaries, to manage failures gracefully.